|  |  |  |  |
| --- | --- | --- | --- |
|  | Job Safety Analysis | | |
| Portland State University | |  |
|  |  |  |
| Facilities Services |  |  |
| Operating a Pedestal Grinder | | |
|  | | |
| **Task** | **Hazards** | **Controls** |
| 1. Check position of tool rest and condition of wheels. | Loose or poorly adjusted tool rests create pinching hazards. | Adjust and tighten tool rests. |
| Cracked or broken wheels create projectile hazards. | Confirm wheels are not cracked or broken. |
| 2. Turn on grinder. | Broken pieces of wheels striking operator | Stand off to the side of the grinder when turning it on. |
| 3. Grind object. | Abrasion and burns to fingers and hands | Wear leather gloves.  Keep fingers and hands away from wheels. |
| Flying sparks and debris | Wear safety glasses or face shield. |
| Pinching hand | Wear leather gloves.  Keep fingers away from pinch points |
| **Required Training:**  1. Operation of grinder | **Required Personal Protective Equipment (PPE)**   1. Leather gloves 2. Safety glasses 3. Face shield | |
|  |  |  |
| **Other Information:** |  | | |
| **Contributors:** | Reviewed JKM | | |
| **Created:** | July 2006 | | |