*This template is a Microsoft Word table – use MS Word’s online “Help” feature for instructions about how to add text and format tables.*

|  |  |
| --- | --- |
|  | Job Safety Analysis |
| Portland State University |  |
|  |  |  |
| Environment, Health & Safety – Chemical Waste |
| Palletizing Drums |
|  |
| **Task** | **Hazards** | **Controls** |
| 1. Tip and roll drum on the edge to the pallet.
 | See “Moving Drums by Hand" JSA. |  |
| 2. Release the drum so that bottom edge rests on pallet. | Hand and finger injury. | Wear heavy gloves.Do not allow hand to be pinched between other drums or objects. |
| Foot injury. | Wear steel-toed boots. |
| 3. Push drum onto the pallet. | Back or muscle strain. | Brace feet firmly.Keep back straight.Keep firm grip on drum top.Get help when available. |
| **Required Training:**Familiarization with this JSA and Task 16. | **Required Personal Protective Equipment (PPE)**Steel-toed boots, lab coat or tyvek suit, safety glasses, and cotton or leather gloves |
|  |  |  |
| **Other Information:** | See “Moving Drums by Hand" JSA. |
| **Contributors:** | Environment, Health & Safety |
| **Created:** | June 2006 |
|  |   |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |